IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView, QuantityTakeOffAddOnView]"
File name: "example.ifc"
Time stamp: "2008-08-01T21:53:56"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "IFC Engine DLL version 1.02 beta"
Originating system: "IFC Engine DLL version 1.02 beta"
Authorization: "The authorising person"
Application: "Test Application" version "0.10" identifier "TA 1001" by Organization "TNO" description "TNO Building Innovation"

People and organizations
  Person "Peter" "Bonsma" id "ID001" of Organization "TNO" description "TNO Building Innovation"
  Owner history of Person "Peter" "Bonsma" id "ID001" of Organization "TNO" description "TNO Building Innovation" | application "Test Application" version "0.10" identifier "TA 1001" by Organization "TNO" description "TNO Building Innovation" | change ADDED | created 1217620436 (2008-08-01T19:53:56Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Default Project" | description "Description of Default Project"
  IFCSITE "Default Site" | latitude 24° 28′ 0″ | longitude 54° 25′ 0″ | description "Description of Default Site"
    IFCBUILDING "Default Building" | description "Description of Default Building"
      IFCBUILDINGSTOREY "Default Building Storey" | elevation 0. | description "Description of Default Building Storey"
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | names: "Wall xyz" | descriptions: "Description of Wall" | material: layers ("Name of the material used for the wall" 3.000E-1) | property sets: Pset_WallCommon, BaseQuantities
          1 x IFCWINDOW | names: "Window xyz" | descriptions: "Description of Window" | property sets: Pset_WindowCommon, BaseQuantities

Property sets
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCTEXT)
    SurfaceSpreadOfFlame = "" (IFCTEXT)
    ThermalTransmittance = 2.400E-1 (IFCREAL)
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 1.500 [SQUARE_METRE]
    GrossSideArea = 11.500 [SQUARE_METRE]
    GrossVolume = 3.450 [CUBIC_METRE]
    Height = 2.300 [METRE]
    Lenght = 5. [METRE]
    NetSideArea = 10.450 [SQUARE_METRE]
    NetVolume = 3.135 [CUBIC_METRE]
    Width = 3.000E-1 [METRE]
  BaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 3.000E-1 [METRE]
    Height = 1.400 [METRE]
    Width = 7.500E-1 [METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Height = 1.400 [METRE]
    Width = 7.500E-1 [METRE]
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCTEXT)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCTEXT)
    GlazingAresFraction = 7.000E-1 (IFCREAL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    Infiltration = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "" (IFCTEXT)
    SecurityRating = "" (IFCTEXT)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 2.400E-1 (IFCREAL)